Displaying the FT-2000 Microphone settings database:

**1**[2](http://www.ft-2000.com/viewmic.php?page=2&mic=Heil%20Pro%20Set) [3](http://www.ft-2000.com/viewmic.php?page=3&mic=Heil%20Pro%20Set) [4](http://www.ft-2000.com/viewmic.php?page=4&mic=Heil%20Pro%20Set) [5](http://www.ft-2000.com/viewmic.php?page=5&mic=Heil%20Pro%20Set) [6](http://www.ft-2000.com/viewmic.php?page=6&mic=Heil%20Pro%20Set) [7](http://www.ft-2000.com/viewmic.php?page=7&mic=Heil%20Pro%20Set) **[Next Settings](http://www.ft-2000.com/viewmic.php?page=2&mic=Heil%20Pro%20Set)**

|  |  |  |  |
| --- | --- | --- | --- |
| Filter by Microphone

|  |  |  |
| --- | --- | --- |
| Select Microphone:  |  |  |

 |
| Callsign: | Setting Name: | Microphone used: |
| PA5CA | Frans | Heil Pro Set |
| Menu 085 TX BPF: |
| 3000 |
| Menu 125 EQ 1 Frequency: | Menu 126 EQ 1 Level: | Menu 127 EQ 1 Bandwidth: |
| 200 | 2 | 8 |
| Menu 128 EQ 2 Frequency: | Menu 129 EQ 2 Level: | Menu 130 EQ 2 Bandwidth: |
| 900 | 2 | 6 |
| Menu 131 EQ 3 Frequency: | Menu 132 EQ3 Level: | Menu 133 EQ 3 Bandwidth: |
| 2100 | 2 | 8 |
| Menu 134 PE 1 Frequency: | Menu 135 PE 1 Level: | Menu 136 PE 1 Bandwidth: |
| 200 | 2 | 8 |
| Menu 137 PE 2 Frequency: | Menu 138 PE 2 Level: | Menu 139 PE 2 Bandwidth: |
| 900 | 2 | 6 |
| Menu 140 PE 3 Frequency: | Menu 141 PE 3 Level: | Menu 142 PE 3 Bandwidth: |
| 2100 | 2 | 8 |
| Mic Gain set at: | Proc Gain set at: |  |
|  |  |  |
| FT-2000 (D) Serial Number: | EDSP Version used: | Firmware Version used: |
| 6J | 1153 | 1.42 |
| Notes about these settings: |
| Works fine with me, I use a Heil HC5 element |

==============================================================================================

Displaying the FT-2000 Microphone settings database:

[**Prev Settings**](http://www.ft-2000.com/viewmic.php?page=2&mic=Heil%20Pro%20Set) [1](http://www.ft-2000.com/viewmic.php?page=1&mic=Heil%20Pro%20Set) [2](http://www.ft-2000.com/viewmic.php?page=2&mic=Heil%20Pro%20Set) **3**[4](http://www.ft-2000.com/viewmic.php?page=4&mic=Heil%20Pro%20Set) [5](http://www.ft-2000.com/viewmic.php?page=5&mic=Heil%20Pro%20Set) [6](http://www.ft-2000.com/viewmic.php?page=6&mic=Heil%20Pro%20Set) [7](http://www.ft-2000.com/viewmic.php?page=7&mic=Heil%20Pro%20Set) [8](http://www.ft-2000.com/viewmic.php?page=8&mic=Heil%20Pro%20Set) [9](http://www.ft-2000.com/viewmic.php?page=9&mic=Heil%20Pro%20Set) **[Next Settings](http://www.ft-2000.com/viewmic.php?page=4&mic=Heil%20Pro%20Set)**

|  |  |  |  |
| --- | --- | --- | --- |
| Filter by Microphone

|  |  |  |
| --- | --- | --- |
| Select Microphone:  |  |  |

 |
| Callsign: | Setting Name: | Microphone used: |
| IW3HXR |  | Heil Pro Set |
| Menu 085 TX BPF: |
| 050-3000 |
| Menu 125 EQ 1 Frequency: | Menu 126 EQ 1 Level: | Menu 127 EQ 1 Bandwidth: |
| 100 | 3 | 6 |
| Menu 128 EQ 2 Frequency: | Menu 129 EQ 2 Level: | Menu 130 EQ 2 Bandwidth: |
| 1500 | 10 | 5 |
| Menu 131 EQ 3 Frequency: | Menu 132 EQ3 Level: | Menu 133 EQ 3 Bandwidth: |
| 3200 | 8 | 4 |
| Menu 134 PE 1 Frequency: | Menu 135 PE 1 Level: | Menu 136 PE 1 Bandwidth: |
| 200 | 3 | 6 |
| Menu 137 PE 2 Frequency: | Menu 138 PE 2 Level: | Menu 139 PE 2 Bandwidth: |
| 1500 | 10 | 5 |
| Menu 140 PE 3 Frequency: | Menu 141 PE 3 Level: | Menu 142 PE 3 Bandwidth: |
| 3200 | 8 | 4 |
| Mic Gain set at: | Proc Gain set at: |  |
|  |  |  |
| FT-2000 (D) Serial Number: | EDSP Version used: | Firmware Version used: |
| 6K070009 | 11.53 | 1.49 |
| Notes about these settings: |
|  |

+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

Displaying the FT-2000 Microphone settings database:

[**Prev Settings**](http://www.ft-2000.com/viewmic.php?page=10&mic=Heil%20Pro%20Set) [6](http://www.ft-2000.com/viewmic.php?page=6&mic=Heil%20Pro%20Set) [7](http://www.ft-2000.com/viewmic.php?page=7&mic=Heil%20Pro%20Set) [8](http://www.ft-2000.com/viewmic.php?page=8&mic=Heil%20Pro%20Set) [9](http://www.ft-2000.com/viewmic.php?page=9&mic=Heil%20Pro%20Set) [10](http://www.ft-2000.com/viewmic.php?page=10&mic=Heil%20Pro%20Set) **11**[12](http://www.ft-2000.com/viewmic.php?page=12&mic=Heil%20Pro%20Set) [13](http://www.ft-2000.com/viewmic.php?page=13&mic=Heil%20Pro%20Set) [14](http://www.ft-2000.com/viewmic.php?page=14&mic=Heil%20Pro%20Set) [15](http://www.ft-2000.com/viewmic.php?page=15&mic=Heil%20Pro%20Set) [16](http://www.ft-2000.com/viewmic.php?page=16&mic=Heil%20Pro%20Set) [17](http://www.ft-2000.com/viewmic.php?page=17&mic=Heil%20Pro%20Set) **[Next Settings](http://www.ft-2000.com/viewmic.php?page=12&mic=Heil%20Pro%20Set)**

|  |  |  |  |
| --- | --- | --- | --- |
| Filter by Microphone

|  |  |  |
| --- | --- | --- |
| Select Microphone:  |  |  |

 |
| Callsign: | Setting Name: | Microphone used: |
| IW3HXR |  | Heil Pro Set |
| Menu 085 TX BPF: |
| 050-3000 |
| Menu 125 EQ 1 Frequency: | Menu 126 EQ 1 Level: | Menu 127 EQ 1 Bandwidth: |
| 100 | 3 | 6 |
| Menu 128 EQ 2 Frequency: | Menu 129 EQ 2 Level: | Menu 130 EQ 2 Bandwidth: |
| 1500 | 10 | 5 |
| Menu 131 EQ 3 Frequency: | Menu 132 EQ3 Level: | Menu 133 EQ 3 Bandwidth: |
| 3200 | 8 | 4 |
| Menu 134 PE 1 Frequency: | Menu 135 PE 1 Level: | Menu 136 PE 1 Bandwidth: |
| 200 | 3 | 6 |
| Menu 137 PE 2 Frequency: | Menu 138 PE 2 Level: | Menu 139 PE 2 Bandwidth: |
| 1500 | 10 | 5 |
| Menu 140 PE 3 Frequency: | Menu 141 PE 3 Level: | Menu 142 PE 3 Bandwidth: |
| 3200 | 8 | 4 |
| Mic Gain set at: | Proc Gain set at: |  |
|  |  |  |
| FT-2000 (D) Serial Number: | EDSP Version used: | Firmware Version used: |
| 6K070009 | 11.53 | 1.49 |
| Notes about these settings: |
|  |

========================================================================================

Displaying the FT-2000 Microphone settings database:

|  |  |  |  |
| --- | --- | --- | --- |
| Filter by Microphone

|  |  |  |
| --- | --- | --- |
| Select Microphone:  |  |  |

 |
| Callsign: | Setting Name: | Microphone used: |
| K4MD |  | Heil Pro Set |
| Menu 085 TX BPF: |
| 050-3000 |
| Menu 125 EQ 1 Frequency: | Menu 126 EQ 1 Level: | Menu 127 EQ 1 Bandwidth: |
| OFF | 30 | 0 |
| Menu 128 EQ 2 Frequency: | Menu 129 EQ 2 Level: | Menu 130 EQ 2 Bandwidth: |
| 1100 | 4 | 0 |
| Menu 131 EQ 3 Frequency: | Menu 132 EQ3 Level: | Menu 133 EQ 3 Bandwidth: |
| 1700 | 5 | 0 |
| Menu 134 PE 1 Frequency: | Menu 135 PE 1 Level: | Menu 136 PE 1 Bandwidth: |
| 200 | 1 | 0 |
| Menu 137 PE 2 Frequency: | Menu 138 PE 2 Level: | Menu 139 PE 2 Bandwidth: |
| 900 | 0 | 0 |
| Menu 140 PE 3 Frequency: | Menu 141 PE 3 Level: | Menu 142 PE 3 Bandwidth: |
| 1900 | 0 | 0 |
| Mic Gain set at: | Proc Gain set at: |  |
| 22 | 52 |  |
| FT-2000 (D) Serial Number: | EDSP Version used: | Firmware Version used: |
|  | 10.29 | 1.38 |
| Notes about these settings: |
|  |  |  |